Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

Motion detector with 360° field of detection for ceiling mounting
Special product features: Zero-cross switching; Simple parameterisation, remote control and documentation with IR-Pen and App; 
User interface: IR remote control
Control system: ON/OFF
Installation type: Surface mounted (plaster)
Installation position: Ceiling
Dimensions: Height/Depth 50 mm, Ø 101 mm
Weight: 113,1 g
Protection type: IP40
Protection class: II
Permissible ambient temperature: 0 °C...+50 °C
Relative humidity: 5–93 %, non-condensing
Colour: white, similar to RAL 9010
Nominal voltage: 230 V AC / 50 Hz
In-rush current: 78 A / 5 ms
Power consumption: 0,2 W
Detection angle: 360°
Detection range diagonally: Ø 8 m
Detection range head-on: Ø 6 m
Field of detection: up to 50 m²
Recommended installation height: 3 m
Max. mounting height: 5 m
Level of brightness: 5–1000 lx
Number of light channels: 1
Slave input: false
Mode: Semi-automatic, Fully automatic
Constant light control: false
Switching delay from "light to dark": 30 s
Switching capacity channel 1: 230 V/50 Hz
2300 W/10 A (cos phi = 1)
1150 VA/5 A (cos phi = 0,5)
600 W LED
Switch contact: make contact / non-floating
Switch-off delay time: 15 s...30 min (adjustable in steps)
Impulse mode: true
Push button input: true