Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

Light control for up to 8 lights with Tunable White

User interface: Push button input, IR remote control
Control system: ELC, DALI
Installation type: Recessed mounting
Installation position: Ceiling
Dimensions: Length 474 mm x Width 345 mm x Height/Depth 140 mm
Weight: 4105 g
Protection type: IP20
Protection class: I
Permissible ambient temperature: 0 °C...+40 °C
Relative humidity: 5–93 %, non-condensing
Colour: white
Nominal voltage: 230 V AC / 60 Hz
Power consumption: 260 W
Number of light channels: 2
Number of light groups: 10
Number of HVAC-channels: 2
Number of scenes: 4
Orientation light: disabled/10–50 %, 2 values can be selected
Constant light control: true
Orientation light duration or time: true
HCL-lighting control: true
Number of outputs luminaires ELC: 8
Number of outputs luminaires DALI: 4