Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

Automatic light with in-built motion detector and 130° field of detection

User interface: Adjusting controller
Control system: ON/OFF
Installation type: Surface mounting
Installation position: Wall
Dimensions: Length 275 mm x Width 185 mm x Height/Depth 250 mm
Weight: 1137 g
Protection type: IP44
Protection class: II
Permissible ambient temperature: -25 °C...+55 °C
Colour: white, similar to RAL 9010
Nominal voltage: 230 V AC / 50 Hz
Diffuser: opal
Light emission: direct
Beam angle: 290 °
Glow wire test in accordance with IEC 60695-2-10: 650 °C

Detection angle: 130° horizontally rotatable

Detection range diagonally: r 12 m

Field of detection: 164 m²

Recommended installation height: 1,8 m

Level of brightness: 5–1000 lx