Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

Design lamp made from die-cast aluminium

Control system: ON/OFF
Installation type: Surface mounting
Installation position: Wall
Dimensions: Length 205 mm x Width 104 mm x Height/Depth 143 mm
Weight: 542,5 g
Protection type: IP55
Protection class: II
Permissible ambient temperature: -25 °C...+50 °C
Colour: white, similar to RAL 9016
Nominal voltage: 230 V AC / 50 Hz
In-rush current: 4,7 A / 33 µs
Diffuser: opal
Light emission: direct
Beam angle: 90 °
Rated output P: 9,5 W
Luminous flux: 850 lm
Luminous efficacy: 89 lm/W
Colour temperature: 3000 K
Colour rendering index Ra: > 80
Rated lifetime L80B50 at 25 °C: 65000 h
Glow wire test in accordance with IEC 60695-2-10: 650 °C