Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

LED DALI bollard light made from high-grade aluminium
Special product features: Integrated motion detector with DALI bus voltage supply; Integrated sensor technology enables energy-efficient control and networking of additional luminaires and switch actuators; Protected against sea air; 
User interface: IR remote control, DALI-Bus
Control system: DALI
Installation type: Free standing
Installation position: Floor
Dimensions: Height/Depth 940 mm, Ø 170 mm
Weight: 7830 g
Protection type: IP65
Protection class: I
Impact resistance: IK09
Permissible ambient temperature: -25 °C...+40 °C
Relative humidity: 5–95 %, non-condensing
Colour: graphite grey, similar to RAL 7024
Nominal voltage: 110 – 240 V AC / 60 Hz
In-rush current: 12 A / 57 µs
Diffuser: opal
Light emission: direct
Beam angle: 283 °
Rated output P: 17 W
Luminous flux: 620 lm
Luminous efficacy: 36 lm/W
Colour temperature: 3100 K
Colour rendering index Ra: > 80
Rated lifetime L80B50 at 25 °C: 70000 h
Photobiological safety: RG0
Detection angle: 140°

Detection range diagonally: r 6 m

Field of detection: 44 m²