Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

High-quality aluminium LED automatic house number light
Special product features: Integrated motion detector; Protected against sea air; 
User interface: IR remote control, Push button input
Control system: ON/OFF
Installation type: Surface mounting
Installation position: Ceiling / wall
Dimensions: Length 250 mm x Width 200 mm x Height/Depth 75 mm
Weight: 1694 g
Protection type: IP65
Protection class: I
Impact resistance: IK09
Permissible ambient temperature: -25 °C...+40 °C
Colour: graphite grey, similar to RAL 7024
Nominal voltage: 230 V AC / 50 Hz
In-rush current: 6 A / 520 µs
Diffuser: opal
Light emission: direct
Beam angle: 120 °
Rated output P: 17 W
Luminous flux: 800 lm
Luminous efficacy: 47 lm/W
Colour temperature: 4000 K
Colour rendering index Ra: > 80
Rated life time L80B50 at 25 °C: 45000 h
Glow wire test in accordance with IEC 60695-2-10: 650 °C

Detection angle: 140°

Detection range diagonally: r 4 m

Field of detection: 20 m²

Recommended installation height: 3 m

Max. mounting height: 5 m