Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

Motion detector with 200° field of detection and modern design
Special product features: One-hand plug-in base; 
User interface: Adjusting controller, IR remote control
Control system: ON/OFF
Installation type: Surface mounting
Installation position: Wall
Dimensions: Height/Depth 55 mm, Ø 110 mm
Weight: 190 g
Protection type: IP55
Protection class: II
Permissible ambient temperature: -25 °C...+55 °C
Relative humidity: 5–95 %, non-condensing
Colour: black, similar to RAL 9005
Nominal voltage: 230 V AC / 50 Hz
In-rush current: 800 A / 200 µs
Power consumption: 0,3 W
Detection angle: 200° (2 x 100° separately adjustable)
Detection range diagonally: Ø 20 m
Detection range head-on: Ø 10 m
Field of detection: up to 175 m²
Recommended installation height: 2,5 m
Max. mounting height: 2,5 m
Level of brightness: 2–2000 lx
Number of light channels: 1
Slave input: false
Constant light control: false
Switching delay from "dark to light": 0 s
Switching delay from "light to dark": 0 s
Switching capacity channel 1: 230 V/50 Hz, 16 AX
2300 W/10 A (cos phi = 1)
1150 VA/5 A (cos phi = 0,5)
600 W LED
Switch contact: make contact / non-floating
Switch-off delay time: 15 s...16 min (adjustable in steps)
Impulse mode: true
Push button input: false