Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

Presence detector with 180° field of detection for wall mounting
Special product features: Simple parameterisation, remote control and documentation with IR-Pen and App; 
User interface: Adjusting controller, IR remote control
Control system: ON/OFF
Installation type: Flush-mounted/Device socket Ø 68 mm
Installation position: Wall
Dimensions: Length 70 mm x Width 70 mm x Height/Depth 55 mm
Installation dimension: Installation depth: 34 mm, Ø 60 mm
Weight: 92 g
Protection type: IP20, IP44 depending on cover (order separately)
Protection class: II
Permissible ambient temperature: 0 °C...+50 °C
Relative humidity: 5–93 %, non-condensing
Colour: opal matt
Nominal voltage: 230 V AC / 50 Hz
In-rush current: 800 A / 200 µs
Power consumption: 1 W
Detection angle: 180° horizontal, 60° vertical
Detection range diagonally: Ø 16 m
Detection range head-on: Ø 6 m
Detection range presence: Ø 4 m
Field of detection: up to 101 m²
Recommended installation height: 1,1 m
Max. mounting height: 2,2 m
Level of brightness: 5–2000 lx
Number of light channels: 1
Number of HVAC-channels: 1
Slave input: true
Max. number of slave detectors: 6
Mode: Semi-automatic, Fully automatic
Constant light control: false
Switching delay from "dark to light": 30 s
Switching delay from "light to dark": 0 s
Switching capacity channel 1: 230 V/50 Hz, 16 AX
2300 W/10 A (cos phi = 1)
1150 VA/5 A (cos phi = 0,5)
600 W LED
Switch contact: make contact / non-floating
Switch-off delay time: 12 s...60 min (adjustable in steps)
Impulse mode: true
Push button input: true