Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

Single-battery emergency light for escape route signage with 3-h emergency light duration for 24-m detection range in accordance with DIN EN 1838

User interface: IR remote control
Control system: ON/OFF
Installation type: Surface mounting
Installation position: Ceiling / wall
Dimensions: Length 328 mm x Width 108 mm x Height/Depth 195 mm
Installation dimension: Installation length: 370 mm x Installation width: 115 mm x Installation depth: 66 mm
Weight: 529 g
Protection type: IP20
Protection class: II
Permissible ambient temperature: 5 °C...+35 °C
Colour: white, similar to RAL 9016
Nominal voltage: 230 V AC / 50 Hz
Light emission: direct
Rated output P: 3 W

Light duration: 3 h
Viewing distance: 24 m
Symbol height: 120 mm
Status display: by LED
Automatic testing: false