Invitation to tender text / Invitation to tender text / Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

LED downlight, 15W, for recessed ceiling mounting with opal diffusor
Control system: DALI

Installation type: Recessed mounting
Installation position: Ceiling
Dimensions: Length 190 mm x Width 165 mm x Height/Depth 57,5 mm
Installation dimension: Installation length: 165 mm x Installation width: 165 mm x Installation depth: 55,5 mm
Weight: 135 g
Protection type: IP20 / IP44 below the ceiling (built-in)
Protection class: II
Permissible ambient temperature: -20 °C...+40 °C
Colour: white, similar to RAL 9003
Nominal voltage: 110 - 240 V AC / 50 - 60 Hz
Diffusor: opal
Light emission: direct
Beam angle: 100 °
Unified Glare Rating: <=28
Rated output P: 16 W
Luminous flux: 1220 lm
Luminous efficacy: 76 lm/W
Colour temperature: 3000 K
Colour rendering index Ra: > 80
Rated life time L80B50 at 25 °C: 40000 h
Glow wire test in accordance with IEC 60695-2-10: 650 °C