Archive / Lighting for indoor areas / Downlights

EO10300509 - IDLELS32009830WHO01-10000

LED downlight, 9 W, for recessed ceiling mounting with opal diffuser
Control system: 1 - 10 V
Installation type: Recessed mounting
Installation position: Ceiling
Dimensions: Length 145 mm x Width 145 mm x Height/Depth 44,5 mm
Installation dimension: Installation length: 125 mm x Installation width: 125 mm x Installation depth: 42,5 mm
Weight: 450 g
Protection type: IP20 / IP44 below the ceiling (built-in)
Protection class: II
Permissible ambient temperature: -20 °C...+40 °C
Colour: white, similar to RAL 9003
Nominal voltage: 110 - 240 V / 50 - 60 Hz
Diffusor: opal
Light emission: direct
Beam angle: 100 °
Unified Glare Rating: <=25
Rated output P: 10 W
Luminous Flux (light): 700 lm
Luminous efficacy: 70,00 lm/W
Colour temperature: 3000 K
Colour rendering index Ra: > 80
Rated life time L80B50 at 25 °C: 40000 h
Glow wire test in accordance with IEC 60695-2-10: 650 °C

opal
direct
100 °
<=25
< 3 %
10 W
false
9 W
700 lm
70,00 lm/W
3000 K
> 80
> 85

40000 h
650 °C
A++ to A
This luminaire contains built-in LED lamps. The lamps in the light cannot be changed.