Archive / Lighting for indoor areas / Downlights

EO10302541 - IDLALI31009830WHT01-10CB0

LED downlight, 9 W, for recessed ceiling mounting with transparent diffuser
Control system: 1 - 10 V
Installation type: Recessed mounting
Installation position: Ceiling
Dimensions: Height/Depth 79 mm, Ø 75 mm
Installation dimension: Installation depth: 77 mm, Ø 68 mm
Weight: 218 g
Protection type: IP20 / IP44 below the ceiling (built-in)
Protection class: II
Permissible ambient temperature: -20 °C...+40 °C
Colour: white, similar to RAL 9003
Nominal voltage: 110 - 240 V / 50 - 60 Hz
Diffusor: transparent
Light emission: direct
Beam angle: 36 °
Unified Glare Rating: <=16
Rated output P: 9 W
Luminous Flux (light): 610 lm
Luminous efficacy: 67,00 lm/W
Colour temperature: 3000 K
Colour rendering index Ra: > 80
Rated life time L80B50 at 25 °C: 55000 h
Glow wire test in accordance with IEC 60695-2-10: 850 °C

transparent
direct
36 °
<=16
< 3 %
9 W
false
8 W
610 lm
67,00 lm/W
3000 K
> 80
85
55000 h
850 °C
A++ to A
This luminaire contains built-in LED lamps. The lamps in the light cannot be changed.