Archive / Lighting for indoor areas / Downlights

EO10304088 - IDLSTI28015830BKT00000000

LED downlight, 15W, for recessed ceiling mounting with transparent diffusor
Control system: ON/OFF
Installation type: Recessed mounting
Installation position: Ceiling
Dimensions: Height/Depth 118,5 mm, Ø 130 mm
Installation dimension: Installation depth: 116,5 mm, Ø 112 mm
Weight: 10 g
Protection type: IP20 / IP44 below the ceiling (built-in)
Protection class: II
Permissible ambient temperature: -20 °C...+40 °C
Colour: Black, similar to RAL 9005
Nominal voltage: 110 - 240 V / 50 - 60 Hz
Diffusor: transparent
Light emission: direct
Beam angle: 60 °
Unified Glare Rating: <=16
Rated output P: 16 W
Luminous Flux (light): 1150 lm
Luminous efficacy: 71,00 lm/W
Colour temperature: 3000 K
Colour rendering index Ra: > 80
Rated life time L80B50 at 25 °C: 60000 h
Glow wire test in accordance with IEC 60695-2-10: 850 °C

transparent
direct
60 °
<=16
< 3 %
16 W
false
15 W
1150 lm
71,00 lm/W
3000 K
> 80
≥ 85

60000 h
850 °C
A++ to A
This luminaire contains built-in LED lamps. The lamps in the light cannot be changed.