Invitation to tender text / Invitation to tender text / Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

LED downlight, 15W, for recessed ceiling mounting with transparent diffusor
Control system: DALI

Installation type: Recessed mounting
Installation position: Ceiling
Dimensions: Height/Depth 118,5 mm, Ø 130 mm
Installation dimension: Installation depth: 116,5 mm, Ø 112 mm
Weight: 476 g
Protection type: IP20 / IP44 below the ceiling (built-in)
Protection class: II
Permissible ambient temperature: -20 °C...+40 °C
Colour: Black, similar to RAL 9005
Nominal voltage: 110 - 240 V AC / 50 - 60 Hz
Diffusor: transparent
Light emission: direct
Beam angle: 60 °
Unified Glare Rating: <=16
Rated output P: 16 W
Luminous flux: 1150 lm
Luminous efficacy: 71 lm/W
Colour temperature: 3000 K
Colour rendering index Ra: > 80
Rated life time L80B50 at 25 °C: 60000 h
Glow wire test in accordance with IEC 60695-2-10: 850 °C