Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

LED office floor light, LED output 45 W, for workplace-oriented lighting in offices and meeting rooms with glare-free direct component and indirect light

User interface: IR remote control, Adjusting controller
Control system: ON/OFF
Installation type: Free standing
Installation position: Floor
Dimensions: Length 600 mm x Width 300 mm x Height/Depth 1950 mm
Weight: 20000 g
Protection type: IP20
Protection class: I
Permissible ambient temperature: 0 °C...+40 °C
Colour: black, similar to RAL 9004
Nominal voltage: 230 V AC / 50 Hz
Diffuser: transparent
Glare suppression: DDP (micro-prismatic)
Light emission: direct/indirect
Beam angle: 90 °
Unified Glare Rating: <=19
Rated output P: 47 W
Luminous flux: 6300 lm
Luminous efficacy: 134 lm/W
Colour temperature: 4000 K
Colour rendering index Ra: > 80
Rated lifetime L80B50 at 25 °C: 70000 h
Photobiological safety: RG0
Detection angle: 360°

Detection range diagonally: Ø 4 m

Detection range head-on: Ø 3 m

Detection range presence: Ø 2 m

Field of detection: 13 m²

Level of brightness: 5–2000 lx