Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

Mini motion detector with 360° field of detection for recessed ceiling mounting for demand-responsive lighting control and therefore noticeable energy cost reductions
Special product features: Simple parameterisation, remote control and documentation with IR-Pen and App; 
User interface: IR remote control
Control system: ON/OFF
Installation type: Recessed mounting
Installation position: Ceiling
Dimensions: Height/Depth 60 mm, Ø 33 mm
Installation dimension: Installation depth: 45 mm, Ø 25 mm
Weight: 287 g
Protection type: IP55
Protection class: II
Permissible ambient temperature: -25 °C...+50 °C
Relative humidity: 5–93 %, non-condensing
Colour: opal matt
Nominal voltage: 230 V AC / 50 Hz
In-rush current: 800 A / 200 µs
Power consumption: 0,2 W
Detection angle: 360°
Detection range diagonally: Ø 8 m
Detection range head-on: Ø 5 m
Field of detection: up to 50 m²
Recommended installation height: 3 m
Max. mounting height: 5 m
Level of brightness: 5–2000 lx
Number of light channels: 1
Slave input: false
Mode: Semi-automatic, Fully automatic
Constant light control: false
Switching delay from "dark to light": 0 s
Switching delay from "light to dark": 30 s
Switching capacity channel 1: 230 V/50 Hz, 16 AX
2300 W/10 A (cos phi = 1)
1150 VA/5 A (cos phi = 0,5)
600 W LED
Switch contact: make contact / non-floating
Switch-off delay time: 60 s...15 min (adjustable in steps)
Impulse mode: true
Push button input: true