Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

Presence detector with 360° field of detection for ceiling mounting
Special product features: Simple parameterisation, remote control and documentation with IR-Pen and App; 
User interface: IR remote control with "blue mode" technology
Control system: ELC
Installation type: Flush-mounted/Device socket Ø 68 mm
Installation position: Ceiling
Dimensions: Height/Depth 70 mm, Ø 108 mm
Installation dimension: Installation depth: 24 mm, Ø 60 mm
Weight: 126 g
Protection type: IP20
Protection class: III
Permissible ambient temperature: -25 °C...+50 °C
Relative humidity: 5–93 %, non-condensing
Colour: white, similar to RAL 9010
Nominal voltage: 9 – 22 V DC
Power consumption: 0,3 W
Detection angle: 360°
Detection range diagonally: Ø 24 m
Detection range head-on: Ø 11 m
Detection range presence: Ø 8 m
Field of detection: up to 453 m²
Recommended installation height: 3 m
Max. mounting height: 5 m
Level of brightness: 5–2000 lx
Number of light channels: 4
Number of HVAC-channels: 2
Slave input: false
Mode: Semi-automatic, Fully automatic
Constant light control: true
Bus system
Switch-off delay time: 60 s...240 min (adjustable in steps)
Impulse mode: false
Push button input: false