Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

Slave presence detector for extending the field of detection of a Master presence detector

User interface: Slide switch (DIP)
Control system: ON/OFF
Installation type: Flush-mounted/Device socket Ø 68 mm
Installation position: Ceiling
Dimensions: Height/Depth 70 mm, Ø 108 mm
Installation dimension: Installation depth: 24 mm, Ø 60 mm
Weight: 140 g
Protection type: IP20
Protection class: II
Permissible ambient temperature: -25 °C...+50 °C
Relative humidity: 5–93 %, non-condensing
Colour: white, similar to RAL 9010
Nominal voltage: 230 V AC / 50 Hz
Power consumption: 0,3 W
Detection angle: 360°
Detection range diagonally: Ø 32 m
Detection range head-on: Ø 11 m
Detection range presence: Ø 8 m
Field of detection: up to 805 m²
Recommended installation height: 3 m
Max. mounting height: 10 m
Slave input: true
Constant light control: false
Bus system
Switch-off delay time: 30 min (adjustable in steps)
Impulse mode: false
Push button input: false