Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

Recessed ceiling mounted KNX presence detector with 360° field of detection
Special product features: Presence and daylight dependent constant light control; Simple parameterisation, remote control and documentation with IR-Pen and App; KNX functions: Alarm, twilight switch, brightness detection, light-dependent motion detection, snooze function, scene telegram via object; 
User interface: IR remote control with "blue mode" technology, ETS-Software
Control system: KNX
Installation type: Flush-mounted/Device socket Ø 68 mm
Installation position: Ceiling
Dimensions: Height/Depth 30 mm, Ø 94 mm
Installation dimension: Installation depth: 24 mm, Ø 60 mm
Weight: 112 g
Protection type: IP20
Protection class: III
Permissible ambient temperature: 5 °C...+35 °C
Relative humidity: 5–93 %, non-condensing
Colour: white, similar to RAL 9010
Nominal voltage: 29 – 31 V DC
Power consumption: 0,2 W
Detection angle: 360°
Detection range diagonally: Ø 8 m
Detection range head-on: Ø 6 m
Detection range presence: Ø 4 m
Field of detection: up to 50 m²
Recommended installation height: 2,5 m
Max. mounting height: 5 m
Level of brightness: 3–1000 lx
Number of light channels: 2
Number of HVAC-channels: 1
Slave input: true
Mode: Semi-automatic, Fully automatic
Constant light control: true
Bus system
Switch-off delay time: 30 s...720 min (adjustable in steps)
Impulse mode: false
Push button input: false