Invitation to tender text / Invitation to tender text / Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

LED light with opal cover (diffuser)
Control system: ELC

Installation type: Insert
Installation position: Ceiling
Dimensions: Length 593 mm x Width 593 mm x Height/Depth 57,6 mm
Installation dimension: Installation length: 600 mm x Installation width: 600 mm x Installation depth: 60 mm
Weight: 5070 g
Protection type: IP20
Protection class: III
Permissible ambient temperature: 0 °C...+40 °C
Colour: white, similar to RAL 9003
Nominal voltage: 42 V DC
Diffusor: opal
Glare suppression: DDP (micro-prismatic)
Light emission: direct
Beam angle: 110 °
Unified Glare Rating: <=19
Rated output P: 32 W
Luminous flux: 3240 lm
Luminous efficacy: 101 lm/W
Colour temperature: 3000 K
Colour rendering index Ra: > 80
Rated life time L80B50 at 25 °C: 70000 h
Glow wire test in accordance with IEC 60695-2-10: 650 °C
Photobiological safety: RG0