Archive / Lighting for indoor areas / Recessed lights

EQ10126284 - PNLCEL14040830WHO00000000

LED light with opal cover (diffuser)
Control system: ON/OFF
Installation type: Insert
Installation position: Ceiling
Dimensions: Length 1195 mm x Width 296 mm x Height/Depth 91 mm
Installation dimension: Installation length: 1200 mm x Installation width: 300 mm x Installation depth: 140 mm
Weight: 4400 g
Protection type: IP20
Protection class: II
Permissible ambient temperature: 0 °C...+40 °C
Relative humidity: 5 - 93 %, non-condensing
Colour: white, similar to RAL 9003
Nominal voltage: 230 V / 50 Hz
Diffusor: semi-opal
Glare suppression: LDP (linear-prismatic)
Light emission: direct
Beam angle: 90 °
Unified Glare Rating: <=19
Rated output P: 46 W
Luminous Flux (light): 4580 lm
Luminous efficacy: 99,00 lm/W
Colour temperature: 3000 K
Colour rendering index Ra: > 80
Rated life time L80B50 at 25 °C: 60000 h
Glow wire test in accordance with IEC 60695-2-10: 650 °C
Photobiological safety: RG0

semi-opal
LDP (linear-prismatic)
direct
90 °
<=19
< 3 %
46 W
false
40 W
4580 lm
99,00 lm/W
3000 K
> 80
> 80
60000 h
650 °C
RG0
A++ to A
This luminaire contains built-in LED lamps. The lamps in the light cannot be changed.