Invitation to tender text / Invitation to tender text / Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

LED light with opal cover (diffuser)
Control system: ELC

Installation type: Insert
Installation position: Ceiling
Dimensions: Length 593 mm x Width 593 mm x Height/Depth 82,6 mm
Installation dimension: Installation length: 600 mm x Installation width: 600 mm x Installation depth: 140 mm
Weight: 5000 g
Protection type: IP20 / IP54 below the ceiling (built-in)
Protection class: III
Permissible ambient temperature: 0 °C...+40 °C
Relative humidity: 5 - 93 %, non-condensing
Colour: white, similar to RAL 9003
Nominal voltage: 42 V DC
Diffusor: opal
Glare suppression: DDP (micro-prismatic)
Light emission: direct
Beam angle: 90 °
Unified Glare Rating: <=19
Rated output P: 32 W
Luminous flux: 3570 lm
Luminous efficacy: 111 lm/W
Colour temperature: 2700 - 6500 K (Tunable White)
Colour rendering index Ra: > 90
Rated life time L80B50 at 25 °C: 70000 h
Glow wire test in accordance with IEC 60695-2-10: 650 °C
Photobiological safety: RG0