Invitation to tender text / Invitation to tender text / Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

LED light set (12x individual lights, controller, presence detector and ISO/IEC11801 2017 cable with RJ45 connector) with opal cover (diffuser)
Control system: ELC

Installation type: Recessed mounting
Installation position: Ceiling
Dimensions: Length 1195 mm x Width 296 mm x Height/Depth 91 mm
Installation dimension: Installation length: 1200 mm x Installation width: 300 mm x Installation depth: 140 mm
Weight: 75000 g
Protection type: IP20
Protection class: I
Permissible ambient temperature: 0 °C...+40 °C
Relative humidity: 5 - 93 %, non-condensing
Colour: white, similar to RAL 9003
Nominal voltage: 230 V AC / 50 Hz
Diffusor: semi-opal
Glare suppression: LDP (linear-prismatic)
Light emission: direct
Beam angle: 90 °
Unified Glare Rating: <=19
Rated output P: 384 W
Luminous Flux (light): 48768 lm
Luminous efficacy: 127,00 lm/W
Colour temperature: 2700 - 6500 K (Tunable White)
Colour rendering index Ra: > 80
Rated life time L80B50 at 25 °C: 60000 h
Glow wire test in accordance with IEC 60695-2-10: 650 °C
Photobiological safety: RG0
Detection angle: 360°
Detection range diagonally: Ø 8 m
Field of detection: 50 m²