Invitation to tender text / Invitation to tender text / Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

LED light with prismatic cover (diffuser)
Control system: ON/OFF

Installation type: Insert
Installation position: Ceiling
Dimensions: Length 296 mm x Width 296 mm x Height/Depth 11 mm
Installation dimension: Installation length: 295 mm x Installation width: 295 mm x Installation depth: 45 mm
Weight: 882 g
Protection type: IP20
Protection class: II
Permissible ambient temperature: 0 °C...+50 °C
Colour: white, similar to RAL 9003
Nominal voltage: 220 - 240 V AC / 50 - 60 Hz
Diffusor: opal
Glare suppression: DDP (micro-prismatic)
Light emission: direct
Beam angle: 100 °
Unified Glare Rating: <=19
Rated output P: 17 W
Luminous flux: 1680 lm
Luminous efficacy: 98 lm/W
Colour temperature: 4000 K
Colour rendering index Ra: > 80
Rated life time L80B50 at 25 °C: 40000 h
Glow wire test in accordance with IEC 60695-2-10: 650 °C
Photobiological safety: RG0