Archive / Lighting for indoor areas / Pendant lights

EV10125331 - PDLPRA04060840STP0DIM0000

LED design pendant light with prismatic cover (diffuser)
Control system: ON/OFF
Installation type: Pendant
Installation position: Ceiling
Dimensions: Length 1200 mm x Width 335 mm x Height/Depth 28 mm
Weight: 9000 g
Protection type: IP20
Protection class: II
Permissible ambient temperature: 0 °C...+40 °C
Colour: chrome
Nominal voltage: 230 V / 50 - 60 Hz
Diffusor: transparent
Glare suppression: DDP (micro-prismatic)
Light emission: direct/indirect
Beam angle: 98 °
Unified Glare Rating: <=16
Rated output P: 60 W
Luminous Flux (light): 6300 lm
Luminous efficacy: 105,00 lm/W
Colour temperature: 4000 K
Colour rendering index Ra: > 80
Rated life time L80B50 at 25 °C: 70000 h
Glow wire test in accordance with IEC 60695-2-10: 650 °C
Photobiological safety: RG0

transparent
DDP (micro-prismatic)
direct/indirect
98 °
<=16
< 3 %
60 W
false
6300 lm
105,00 lm/W
4000 K
> 80
CQS > 80
70000 h
650 °C
RG0
A++ to A
This luminaire contains built-in LED lamps. The lamps in the light cannot be changed.