Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

IR remote control for end users of the DEFENSOR series: Setting the level of brightness, the switch-off delay time (5 or 15 minutes) and light ON/OFF for 12 hours

Dimensions: Length 56 mm x Width 29 mm x Height/Depth 7 mm
Weight: 12 g
Protection type: IP20
Colour: silver